EGR VALVE REMOVAL/INSTALLATION [LF]

#
EGR VALVE REMOVAL/INSTALLATION [LF]

B3E011620300W01

1. Remove the plug hole plate.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [LF].)

3. Disconnect the negative battery cable.

4. Disconnect the EGR valve connector.

5. Remove in the order indicated in the table.

.

1 | Water hose (See Water Hose Removal Note [LF].)
2 | EGR valve (See EGR Valve Removal Note [LF].)

6. Install in the reverse order of removal.

## Water Hose Removal Note [LF]

1. Drain the engine coolant from the radiator. (See ENGINE COOLANT REPLACEMENT.)

## EGR Valve Removal Note [LF]

1. Remove the air cleaner and air hose. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [LF].)

2. Remove the radiator hose (upper). (See RADIATOR REMOVAL/INSTALLATION.)