SHROUD PANEL REMOVAL/INSTALLATION

#
SHROUD PANEL REMOVAL/INSTALLATION

B3E091053580W02

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination lights. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove the front bumper reinforcement. (See FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION.)

5. Remove the bonnet latch. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [L.H.D.], BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [R.H.D.].)

6. Remove in the order indicated in the table.

1 | Radiator mount cap
2 | Bolt
3 | Shroud panel

7. Install in the reverse order of removal.