JACKING POSITIONS, VEHICLE LIFT (2 SUPPORTS) AND SAFETY STAND (RIGID RACK) POSITIONS

#
JACKING POSITIONS, VEHICLE LIFT (2 SUPPORTS) AND SAFETY STAND (RIGID RACK) POSITIONS

B3E000000007W01

## Jacking Positions

  Warning

  • Improperly jacking a vehicle is dangerous. The vehicle can slip off the jack and cause serious injury. Use only the correct front and rear jacking points and block the wheels.

• Use safety stands to support the vehicle after it has been lifted.

### Front

  Note

  • Before setting the jack under the vehicle, place boards (approx. 20 mm {0.78 in} thick) under the front tires so that the bumper does not interfere with the jack.

  • At the center of the front crossmember.

### Rear

  Caution

  • Place a board (approx. 20 mm {0.78 in} thick) between the rear crossmember and the jack to prevent damage to the crossmember.

  • At the center of the rear crossmember.

## Vehicle Lift Positions

### Front and rear

  Warning

  • Unstably lifting a vehicle is dangerous. The vehicle can slip off the lift and cause serious injury and/or vehicle damage. Make sure that the vehicle is on the lift horizontally by adjusting the height of support at the end of the arm of the lift.

## Safety Stand Positions

### Front and rear

  • Both sides of the vehicle, on side sills.