ELECTRIC POWER STEERING OIL PUMP (LF) REMOVAL/INSTALLATION

#
ELECTRIC POWER STEERING OIL PUMP (LF) REMOVAL/INSTALLATION

B3E061432650W02

1. Remove the under cover, splash shield and mudguard.

2. Remove the washer tank. (See WASHER TANK REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

.

1 | Connector
2 | Pressure pipe
3 | Suction hose
4 | Electric power steering oil pump and bracket component
5 | Bracket
6 | Electric power steering oil pump