DTC P0037 [ZJ, Z6]

#
DTC P0037 [ZJ, Z6]

B3E010200001W05

DTC P0037 | Rear HO2S heater control circuit low
--- | ---

DETECTION CONDITION

• The PCM monitors the rear HO2S heater control voltage at PCM terminal 2AT. If the PCM turns the rear HO2S heater off but the rear HO2S heater circuit has low voltage, the PCM determines that the rear HO2S heater circuit has a malfunction.
Diagnostic support note
• This is a continuous monitor (HO2S heater).
• The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle.
• FREEZE FRAME DATA is available.
• The DTC is stored in the PCM memory.

POSSIBLE CAUSE

• Rear HO2S heater malfunction
• Open circuit in wiring harness between rear HO2S terminal C and PCM terminal 2T
• Open circuit in wiring harness between rear HO2S terminal D and PCM terminal 2AT
• Short to GND in wiring harness between rear HO2S terminal D and PCM terminal 2AT
• Connector or terminal malfunction
• PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT REAR HO2S CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the rear HO2S connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
4 | INSPECT REAR HO2S HEATER • Inspect the rear HO2S heater. (See REAR HEATED OXYGEN SENSOR (HO2S) INSPECTION [ZJ, Z6].) • Is there any malfunction? | Yes | Replace the rear HO2S, then go to Step 9. (See REAR HEATED OXYGEN SENSOR (HO2S) REMOVAL/INSTALLATION [ZJ, Z6].)
No | Go to the next step.
5 | INSPECT REAR HO2S HEATER POWER CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for continuity between rear HO2S terminal C (wiring harness-side) and PCM terminal 2T (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to Step 9.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
7 | INSPECT REAR HO2S CIRCUIT FOR SHORT TO GND • Turn the ignition switch off. • Inspect for continuity between rear HO2S terminal D (wiring harness-side) and body GND. • Is there continuity? | Yes | Repair or replace the wiring harness for a possible short to GND, then go to Step 9.
No | Go to the next step.
8 | INSPECT REAR HO2S CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch off. • Inspect for continuity between rear HO2S terminal D (wiring harness-side) and PCM terminal 2AT (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to the next step.

9

VERIFY TROUBLESHOOTING OF DTC P0037 COMPLETED
• Make sure to reconnect all disconnected connectors.
• Clear the DTC from the PCM memory using the WDS or equivalent.
• Perform the "HO2S heater, HO2S, and TWC Repair Verification Drive Mode".
(See OBD DRIVE MODE [ZJ, Z6].)
• Is the PENDING CODE for this DTC present?

Yes

Replace the PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [ZJ, Z6].)

No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [ZJ, Z6].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [ZJ, Z6].)
No | DTC troubleshooting completed.