NO.11 SHIFT POINT IS HIGH OR LOW

#
NO.11 SHIFT POINT IS HIGH OR LOW

B3E050319090W15

11 | Shift point is high or low
DESCRIPTION | • Shift point considerably different from automatic shift diagram. • Shift delays when accelerating. • Shift occurs quickly when accelerating and engine speed does not increase.

POSSIBLE CAUSE

• If the transaxle does not shift abnormally, there is a malfunction of the input signal to the TP sensor, input/turbine speed sensor, or vehicle speed sensor (including sensor GND).
• If the engine speed is high or low, regardless of normal shifting, inspect the tachometer.
• Verify that the output signal of the TP sensor changes linearly.