SIDE PROTECTOR INSTALLATION

#
SIDE PROTECTOR INSTALLATION

B3E091650680W02

1. Remove the adhesive remaining on the side protector and the body using a razor.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

2. Remove any grease or dirt from the adhesion surface of the side protector and the body.

3. Attach double-sided adhesive tape to the side protector as shown in the figure.

  Clearance
  a: 30 mm {1.2 in}
  b: 2.0 mm {0.08 in}
  c: 12 mm {0.47 in}
  d: 3.0 mm {0.12 in}
  e: 3.0 mm {0.12 in}
  f: 1.0-3.0 mm {0.04-0.11 in}
  g: 5.0 mm {0.2 in}
  h: 1.0 mm {0.04 in}

4. Peel off the backing paper from the double-sided adhesive tape and attach the side protector onto the body as shown in the figure.

  Clearance
  a: 1.4-4.4 mm {0.056-0.17 in}
  b: 3.0-6.0 mm {0.12-0.23 in}