REAR COMBINATION LIGHT REMOVAL/INSTALLATION

#
REAR COMBINATION LIGHT REMOVAL/INSTALLATION

B3E091851150W01

1. Disconnect the negative battery cable.

2. Remove the trunk end trim. (4SD) (See TRUNK END TRIM REMOVAL/INSTALLATION.)

3. Remove the fasteners and slightly bend back the trunk side trim. (4SD)

4. Remove the service hole cover. (5HB)

5. Remove in the order indicated in the table.

1 | Nut
2 | Connector
3 | Rear combination light
4 | Socket
5 | Rear turn light bulb
6 | Brake light/taillight bulb

6. Install in the reverse order of removal.