STEERING GEAR AND LINKAGE INSPECTION

#
STEERING GEAR AND LINKAGE INSPECTION

B3E061432960W03

## Steering Rack Inspection

1. Inspect for cracking, damage, and tooth wear.

  • If there is any malfunction, replace the steering rack.

2. Measure the steering rack warp.

  • If it exceeds the maximum specification, replace the steering rack.

  Minimum
  Near point A: 0.15 mm {0.006 in}
  Near point B: 0.20 mm {0.008 in}

## Tie-rod End Inspection

1. Inspect the tie-rod end for damage and the boot for cracks.

  • If there is any malfunction, replace the tie-rod end.

2. Inspect for excessive play.

  • If there is any malfunction, replace the tie-rod end.

3. Rotate the ball joint 10 times.

4. Install two nuts to the ball joint and measure the tie-rod end rotational torque using a torque wrench.

  • If not within the specification, replace the tie-rod end.

  Standard rotational torque
  0.5-3.0 N·m {6-30 kgf·cm, 5-26 in·lbf}

## Tie rod Inspection

1. Inspect for bending and damage.

  • If there is any malfunction, replace the tie rod.

2.• Inspect for excessive play.

  • If there is any malfunction, replace the tie rod.

3. Swing the ball joint 10 times.

4. Measure the ball joint swing torque using a pull scale.

  • If it exceeds the specification, replace the tie rod.

  Standard swing torque
  0.4-4.0 N·m {5-40 kgf·cm, 4-35 in·lbf}
  Pull scale reading
  0.6-29.3 N {0.06-2.98 kgf, 0.14-6.58 lbf}