FRONT SHOCK ABSORBER INSPECTION

#
FRONT SHOCK ABSORBER INSPECTION

B3E021334700W01

1. Remove the front shock absorber.

2. Inspect for damage and oil leakage.

3. Compress and extend the shock absorber piston rod at least three times at a steady rate. From the fourth compression stroke, verify that the operational force does not change and that there is no unusual noise.

  • If there is any malfunction, replace the shock absorber.