CLUTCH COVER INSPECTION

#
CLUTCH COVER INSPECTION

B3E051016410W01

1. Measure the wear of the diaphragm spring fingers.

  • If it exceeds the maximum specification, replace the clutch cover.

  Maximum depth
  0.6 mm {0.024 in}

2. Measure the flatness of the pressure plate with a straight edge and a feeler gauge.

  • If it exceeds the maximum specification, replace the clutch cover.

  Maximum clearance
  0.5 mm {0.020 in}

3. When checking the diaphragm spring fingers, mount a dial indicator on the cylinder block.

4. Rotate the flywheel and check for misaligned diaphragm spring fingers.

  • If it exceeds the maximum specification, replace the clutch cover.

  Maximum height difference
  1.0 mm {0.039 in}