BATTERY REMOVAL/INSTALLATION [ZJ, Z6]

#
BATTERY REMOVAL/INSTALLATION [ZJ, Z6]

B3E011718520W01

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

.

1 | Battery cover (See Battery Cover Installation Note.)
2 | Negative battery cable
3 | Positive battery cable
4 | Battery box (See Battery Box Installation Note.)
5 | Battery clamp
6 | Battery
7 | Battery tray

## Battery Box Installation Note

1. Assemble with the battery box hooks E aligned with the battery tray holes at two points.

## Battery Cover Installation Note

1. Install with the battery cover hooks A aligned with the battery tray holes at two points.

2. Install with the battery cover hooks D aligned with the battery tray flange at two points.

3. Set the battery cover to the battery tray hooks C at two points.