PID/DATA MONITOR TABLE

#
PID/DATA MONITOR TABLE

B3E080201046W07

PID name (definition) | Unit/Condition | Operation Condition (Reference) | Terminal
--- | --- | --- | ---
CCNT_RCM (Number of continuous DTCs) |  | • DTCs detected: 1-255 • No DTCs detected: 0 |
D_ABAGR2 (Driver-side air bag module (inflator No.2) resistance) | Ohm | Under any condition: 1.5-3.7 ohms | 1U, 1Q
DABAGR (Driver-side air bag module (inflator No.1) resistance) | Ohm | Under any condition: 1.5-3.7 ohms | 1I, 1M
DFCURTRES (Driver-side curtain air bag module resistance) | Ohm | Under any condition: 1.4-3.2 ohms | 2AG, 2AK
DR_BUKL (Driver-side buckle switch status) | Buckled/ Unbuckled | • Driver-side buckle switch on: Buckled • Driver-side buckle switch off: Unbuckled | 2W
DR_PTENS (Driver-side pre-tensioner front buckle resistance) | Ohm | Under any condition: 1.5-3.1 ohms | 2J, 2N
DS_AB (Driver-side side air bag module resistance) | Ohm | Under any condition: 1.4-3.2 ohms | 2B, 2F
I_PAD_FLT (PAD switch status) | OK/ Fault | • PAD switch normal: OK • PAD switch abnormal: Fault | 1P
I_PAD_SW (PAD switch status) | ON/ OFF | • PAD switch is at PASS AIRBAG ON position: ON • PAD switch is at PASS AIRBAG OFF position: OFF | 1P
P_ABAGR2 (Passenger-side air bag module (inflator No.2) resistance) | Ohm | Under any condition: 1.4-2.9 ohms | 1R, 1V
PABAGR (Passenger-side air bag module (inflator No.1) resistance) | Ohm | Under any condition: 1.4-2.9 ohms | 1J, 1N
PFCURTRES (Passenger-side curtain air bag module resistance) | Ohm | Under any condition: 1.4-3.2 ohms | 2AH, 2AL
PS_AB (Passenger-side side air bag module resistance) | Ohm | Under any condition: 1.4-3.2 ohms | 2I, 2M
PS_PTENS (Passenger-side pre-tensioner front buckle resistance) | Ohm | Under any condition: 1.5-3.1 ohms | 2A, 2E
VBATTRCM (SAS control module input voltage) | V | • Ignition switch is at ON: B+ • Other: 0 | 1D