FRONT DOOR LOCK ACTUATOR INSPECTION

#
FRONT DOOR LOCK ACTUATOR INSPECTION

B3E091458490W06

1. Apply battery positive voltage and connect ground to the corresponding front door lock actuator terminals, and inspect the front door lock actuator operation.

  • If not as specified, replace the front door latch and lock actuator.

Lock actuator operation | Connection
--- | ---
B+ | GND
Double lock | H | LH: C RH: D
Lock | LH: D RH: C | LH: C RH: D
Unlock | LH: C RH: D | LH: D RH: C