FRONT DOOR REMOVAL/INSTALLATION

#
FRONT DOOR REMOVAL/INSTALLATION

B3E091158010W02

1. Disconnect the negative battery cable.

2. To remove the checker, remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)
  (2) Regulator handle (Vehicles with manual window system) (See REGULATOR HANDLE REMOVAL.) (See REGULATOR HANDLE INSTALLATION.)
  (3) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)
  (4) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

3. To remove the front door hinges, remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)
  (2) Cowl grille (See COWL GRILLE REMOVAL/INSTALLATION.)
  (3) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)
  (4) Front combination lights (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)
  (5) Side step molding (Vehicle with the side step molding) (See SIDE STEP MOLDING REMOVAL/INSTALLATION.)
  (6) Front fender panel (See FRONT FENDER PANEL REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

5. Adjust the front door. (See DOOR ADJUSTMENT.)

6. Install in the reverse order of removal.

.

1 | Connector (See Connector Removal Note.)
2 | Bolt A
3 | Bolt B
4 | Front door
5 | Bolt C
6 | Checker
7 | Bolt D
8 | Front door hinge

## Connector Removal Note

1. Pull down the lever in the direction indicated by the arrow and disconnect the connector.