REAR PACKAGE TRIM REMOVAL/INSTALLATION

#
REAR PACKAGE TRIM REMOVAL/INSTALLATION

B3E091768300W01

1. Remove the following parts:

  (1) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

2. Remove the fasteners.

3. Pull the rear package trim upward and detach clips A and locator pin B from the body.

4. Detach tabs C from the body and remove the rear package trim.

5. Install in the reverse order of removal.