IGNITION SWITCH REMOVAL/INSTALLATION

#
IGNITION SWITCH REMOVAL/INSTALLATION

B3E092166151W01

1. Disconnect the negative battery cable.

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Ignition switch
2 | Connector (See Connector Removal Note.) (See Connector Installation Note.)

4. Install in the reverse order of removal.

## Connector Removal Note

1. Rotate the lever in the direction of the arrow and remove the connector.

## Connector Installation Note

1. After connecting the connector, rotate the lever in the direction of the arrow to install the connector.