ROOF CARRIER BRACKET REMOVAL/INSTALLATION

#
ROOF CARRIER BRACKET REMOVAL/INSTALLATION

B3E091670600W01

1. Remove the following parts:

  (1) Console (4SD) (See CONSOLE REMOVAL/INSTALLATION.)
  (2) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (3) Upper anchor of the front seat belt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  (4) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (5) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)
  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)
  (8) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (9) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (10) Trunk side upper trim (5HB) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION.)
  (11) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)
  (12) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (13) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (14) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (15) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (16) Headliner (See HEADLINER REMOVAL/INSTALLATION.)
  (17) Roof molding (See ROOF MOLDING REMOVAL.) (SeeROOF MOLDING INSTALLATION.)

2. Remove the nuts.

3. Remove the roof carrier bracket.

4. Install in the reverse order of removal.

  Note

  • Install the roof carrier bracket so that the arrow on it faces inward.