REAR DOOR QUARTER GLASS REMOVAL/INSTALLATION

#
REAR DOOR QUARTER GLASS REMOVAL/INSTALLATION

B3E091259500W03

1. Disconnect the negative battery cable. (Vehicles with power window system)

2. Remove the rear beltline molding. (See REAR BELTLINE MOLDING REMOVAL/INSTALLATION.)

3. Remove the regulator handle. (Vehicles with manual window system) (See REGULATOR HANDLE REMOVAL.)

4. Remove the rear door trim. (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

5. Remove the bolts and screw.

6. Remove the rear door glass guide and glass run channel as a single unit.

7. Remove the rear door quarter glass.

8. Install in the reverse order of removal.