MASTER CYLINDER REMOVAL/INSTALLATION

#
MASTER CYLINDER REMOVAL/INSTALLATION

B3E041143400W02

1. For L.H.D., remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

.

1 | Brake fluid level sensor connector
2 | Reserve hose (MTX) (See Reserve Hose Removal Note.) (See Reserve Hose Installation Note.)
3 | Brake pipe
4 | Nut
5 | Master cylinder
6 | Reserve tank, cap

## Reserve Hose Removal Note

1. Remove the reserve hose from the reserve tank while pressing the point indicated by the arrow in the figure.

## Reserve Hose Installation Note

1. Insert the reserve hose to the reserve tank until a click is heard.

2. Verify that the reserve hose is firmly installed by pulling it, and push it into the reserve tank again.