NEUTRAL SWITCH REMOVAL/INSTALLATION [G35M-R]

#
NEUTRAL SWITCH REMOVAL/INSTALLATION [G35M-R]

B3E051501029W06

1. Remove the under cover.

2. Remove the No.1 engine mount rubber and No.1 engine mount bracket.

3. Remove the neutral switch.

4. Install the neutral switch (with a new packing) to the transmission case.

  Tightening torque
  19.6-29.4 N·m
  {2.0-2.9 kgf·m, 14.5-21.6 ft·lbf}

5. Install the No.1 engine mount bracket and No.1 engine mount rubber.