REAR WIPER MOTOR REMOVAL/INSTALLATION

#
REAR WIPER MOTOR REMOVAL/INSTALLATION

B3E091967450W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Rear wiper arm and blade (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION.)
  (2) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)
  (3) Liftgate side trim (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)
  (4) Liftgate lower trim (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

3. Disconnect the rear wiper motor connector.

4. Remove the bolts, then remove the rear wiper motor.

5. Remove the outer bushing.

6. Install in the reverse order of removal.