AIR INTAKE ACTUATOR REMOVAL/INSTALLATION

#
AIR INTAKE ACTUATOR REMOVAL/INSTALLATION

B3E074061060W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front scuff plate (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (2) Front side trim (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (3) Decoration panel (SeeDECORATION PANEL REMOVAL/INSTALLATION.)
  (4) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (5) Car-navigation unit (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

3. Slide the blower case to the position shown in the figure. (See BLOWER MOTOR REMOVAL.) (R.H.D.)

4. Remove in the order indicated in the table.

L.H.D.

R.H.D.

1 | Air intake actuator connector
2 | Air intake actuator

5. Install in the reverse order of removal.