AUDIO CONTROL SWITCH INSPECTION

#
AUDIO CONTROL SWITCH INSPECTION

B3E092000148W02

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module.(See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the audio control switch connector.

4. Verify the resistance and continuity between the audio control switch terminals.

  • If the resistance and continuity are not as indicated in the tables, replace the audio control light switch.

  R: :
Resistance.See the table.

Switch position | Resistance (ohm)
--- | ---
VOL- button ON | 51-56
VOL+ button ON | 140-154
AUTO SCAN button ON | 286-315
PRESET button ON | 534-589
MODE button ON | 985-1,080
MUTE button ON | 1,940-2,130
OFF | 4,800-5,290