FRONT DOOR SPEAKER REMOVAL/INSTALLATION

#
FRONT DOOR SPEAKER REMOVAL/INSTALLATION

B3E092066961W01

1. Disconnect the negative battery cable.

2. Remove the front door trim.(See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Front door speaker (See Front Door Speaker Installation Note.)

4. Install in the reverse order of removal.

## Front Door Speaker Installation Note

1. Remove the speaker with the wiring harness passing through the groove of the front door module.

  Caution

  • If the speaker is installed with the wiring harness out of the groove, an open circuit in the wiring harness could occur.