REAR WHEEL ALIGNMENT

#
REAR WHEEL ALIGNMENT

B3E021101016W01

## Specification (Unloaded)*1

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | Tire [Tolerance ±4 {±0.16}] | (mm {in}) | 2 {0.08}
Rim inner | 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Camber angle*2 (Reference value) [Tolerance ±1°] | -1°10' | -1°12' | -1°14' | -1°17' | -1°19'
Thrust angle (Reference value) [Tolerance ±0°48'] | 0°

  *1 :
Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
  *2 :
Difference between left and right must not exceed 1°30' .

  Note

Total toe-in measuring position

  • Tire: A indicated in the figure (between the center of the tires)
  • Rim inner: B indicated in the figure (between the inner side of the rims)

## Total Toe-in Adjustment

1. Loosen the installation nut of the adjusting cam bolt.

2. Rotate the adjusting cam bolt in either direction to adjust the camber.

| Left wheel | Right wheel
--- | --- | ---
Toe-out direction | Clockwise | Counterclockwise
Toe-in direction | Counterclockwise | Clockwise

3. Tighten the nut.

  Tightening torque
  80.0-100.0 N·m {8.16-10.19 kgf·m, 59.01-73.75 ft·lbf}