DTC 00:ER01

#
DTC 00:ER01

B3E090266900W14

DTC 00:Er01 | Cassette deck
DETECTION CONDITION | • Cassette deck cannot implement insert and eject commands.
POSSIBLE CAUSE | • Defective cassette tape (deformation, broken, or foreign material stuck/attached) • Cassette deck malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Can cassette tape be ejected? | Yes | Go to the next step.
No | Replace the cassette deck.
2 | Verify condition of the cassette tape when the error occurs. Is the cassette tape normal? | Yes | Go to the next step.
No | Repair (remove foreign material) or replace the cassette tape, and go to the next step.
3 | Clear the DTC. Insert then eject a normal cassette tape. Is DTC 00: Er01 displayed? | Yes | Replace the cassette deck.
No | DTC troubleshooting completed.