AIR FILTER REMOVAL/INSTALLATION

#
AIR FILTER REMOVAL/INSTALLATION

B3E071113988W01

1. Disconnect the negative battery cable.

2. Remove the PJB and PJB bracket. (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)

3. Remove the side wall.

4. Disconnect the evaporator temperature sensor connector (L.H.D.).

5. Disconnect the power MOS FET connector. (L.H.D. Full-auto air conditioner)

6. Remove in the order indicated in the table.

L.H.D.

R.H.D.

1 | Air filter cover
2 | Air filter (1)
3 | Air filter (2)

7. Install in the reverse order of removal.