DTC 06:ER01

#
DTC 06:ER01

B3E090266900W17

DTC 06:Er01 | CD changer (upper module)
DETECTION CONDITION | • CD changer (upper module) cannot implement insert, eject, and disc change commands.
POSSIBLE CAUSE | • Defective CD (broken or foreign material stuck/attached) • CD changer (upper module) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Can CD be ejected? | Yes | Go to the next step.
No | Replace the CD changer (upper module).
2 | Verify the condition of the CD when the error occurs. Is the CD normal? | Yes | Go to the next step.
No | Repair (remove foreign material) or replace the CD, and go to the next step.
3 | Clear the DTC. Insert then eject a normal CD. Is DTC 06: Er01 displayed? | Yes | Replace the CD changer (upper module).
No | DTC troubleshooting completed.