DTC B105A

#
DTC B105A

B3E080201046W30

DTC B105A | SAS control module activation (deployment) control frequency error
--- | ---

DETECTION CONDITION

  Warning

  • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure.

• The SAS control module has enabled the air bag module or pre-tensioner front buckle to operate (deploy) five times or more.

POSSIBLE CAUSE | • SAS control module malfunction

Diagnostic procedure

ACTION
• Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)