NO.29 DOES NOT UPSHIFT IN M RANGE

#
NO.29 DOES NOT UPSHIFT IN M RANGE

B3E050319090W33

29 | Does not upshift in M range
DESCRIPTION | • Gear position indicator light in instrument cluster illuminates, but the vehicle does not upshift when the selector lever is pushed to "+" side.

POSSIBLE CAUSE

• Up switch or related wiring harness malfunction

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Inspect the UP SW PID value using the WDS or equivalent. (See PCM INSPECTION [ZJ, Z6].) (See PCM INSPECTION [LF].) Is the UP SW PID value normal? | Yes | Inspect the instrument cluster.
No | Inspect the up switch. If the up switch is normal, inspect for continuity between the up switch and PCM terminal 1P.

2

• Verify the test results.

  - If normal, return to the diagnostic index to service any additional symptoms.
  - If the malfunction remains, inspect the related Service information and perform repair or diagnosis.

  • If the vehicle is repaired, troubleshooting is completed.
  • If the vehicle is not repaired or additional diagnostic information is not available, replace the PCM.