DISCHARGE HEADLIGHT SYSTEM INSPECTION

#
DISCHARGE HEADLIGHT SYSTEM INSPECTION

B3E091851030W04

## Discharge Headlight Inoperative

  Warning

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

Terminal layout

Inspection procedure

STEP | INSPECTION | ACTION
--- | --- | ---

1

INSPECT POWER SUPPLY CIRCUIT OF DISCHARGE HEADLIGHT CONTROL MODULE
• Disconnect the discharge headlight control module connector.
• Turn the headlight switch to the HEADLIGHT (LO) position.
• Measure the voltage at discharge headlight control module terminal A (wiring harness-side).
• Is the voltage approx. 12 V?

Yes

Go to Step 6.

No | Go to the next step.
2 | INSPECT FUSE • Turn the headlight switch to the OFF position. • Remove the HEAD LOW R 15 A fuse (RH) or HEAD LOW L 15 A fuse (LH). • Inspect the fuses. • Are the fuses normal? | Yes | Go to the next step.
No | Replace the fuse.
3 | INSPECT HEADLIGHT RELAY • Inspect the PJB. (See PASSENGER JUNCTION BOX (PJB) INSPECTION.) • Is the headlight relay normal? | Yes | Go to the next step.
No | Replace the PJB. (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)
4 | INSPECT LIGHT SWITCH • Inspect the light switch. (See LIGHT SWITCH INSPECTION.) • Is the light switch normal? | Yes | Go to the next step.
No | Replace the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

5

INSPECT WIRING HARNESS BETWEEN BATTERY AND DISCHARGE HEADLIGHT CONTROL MODULE
• Disconnect the negative battery cable.
• Inspect for continuity between the following terminals:

  - Battery (positive terminal) and PJB (terminal J-01 AM)
  - HEAD LOW R 15 A fuse (RH) and discharge headlight control module terminal A
  - HEAD LOW L 15 A fuse (LH) discharge headlight control module terminal A

• Are the wiring harnesses normal?

Yes

Go to the next step.

No | Replace the related wiring harness.

6

INSPECT WIRING HARNESS BETWEEN DISCHARGE HEADLIGHT CONTROL MODULE AND GROUND
• Inspect the wiring harness between discharge headlight control module terminal B and ground for the following:

  - Short to power supply
  - Open circuit

• Is the wiring harness normal?

Yes

Go to the next step.

No | Replace the related wiring harness.

7

VERIFY WHETHER MALFUNCTION IS IN DISCHARGE HEADLIGHT BULB OR DISCHARGE HEADLIGHT CONTROL MODULE
• Install any other discharge headlight bulb (low-beam). (See HEADLIGHT BULB REMOVAL/INSTALLATION.)
• Connect the discharge headlight control module connector.
• Turn the headlight switch to the HEADLIGHT (LO) position.
• Does the headlight (low-beam) illuminate?

Yes

System inspection completed.

No | Replace the discharge headlight control module. (See DISCHARGE HEADLIGHT CONTROL MODULE REMOVAL/INSTALLATION.)