DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM]

#
DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM]

B3E090255430W02

DTC | Malfunction location | DTC output module | Page
--- | --- | --- | ---
U0073 | CAN system communication error | • PCM • EHPAS control module • Instrument cluster | (See DTC U0073, U2012.)
SAS control module | (See DTC U0073, U0516, U1900, U2516.)
U0100 | Communication error to PCM | • EHPAS control module • Instrument cluster | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)
U0121 | Communication error to DSC HU/CM or ABS HU/CM | • PCM • Instrument cluster
U0131 | Communication error to EHPAS control module | Instrument cluster
U0140 | Communication error to PJB | • Instrument cluster • Climate control unit
U0151 | Communication error to SAS control module | Instrument cluster
U0155 | Communication error to instrument cluster | • PCM • Climate control unit
U0184 | Communication error to audio unit (base module) | • Instrument cluster • Climate control unit
U0516 | CAN system communication error | Climate control unit | (See DTC U0073, U0516, U1900, U2516.)
U1900 | Communication error to PCM | • ABS HU/CM (with ABS) • DSC HU/CM (with DSC) | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)
Communication error to instrument cluster | SAS control module
CAN system communication error Abnormal message from other modules | PJB | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.) (See DTC U0073, U0516, U1900, U2516.)
U2012 | CAN system communication error | • ABS HU/CM (with ABS) • DSC HU/CM (with DSC) | (See DTC U0073, U2012.)
U2023 | Abnormal message from PCM | EHPAS control module | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)
U2202 | Communication error to PCM | DSC HU/CM (with DSC) | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)
U2516 | CAN system communication error | Instrument cluster | (See DTC U0073, U0516, U1900, U2516.)
U2523 | Communication error to PCM | • ABS HU/CM (with ABS) • DSC HU/CM (with DSC) | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)