STEERING SHAFT INSPECTION

#
STEERING SHAFT INSPECTION

B3E061432100W01

1. Inspect the column bearing for excessive play and damage.

2. Verify that the measurement of the steering shaft indicated in the figure is as specified.

  • If not within the specification replace the steering shaft component.

  Standard
  315-320 mm {12.41-12.59 in}

3. Inspect the tilt/telescope mechanism operation for the following.

  (1) Tilt/telescope lever moves smoothly from the lock to the unlock position.
  (2) Steering shaft is fixed firmly when the tilt/telescope lever is locked.

  • If there is any malfunction, replace the steering shaft.