REAR SPOILER REMOVAL/INSTALLATION

#
REAR SPOILER REMOVAL/INSTALLATION

B3E091651960W01

## 4SD

1. Remove the nuts.

2. While cutting the double-sided adhesive tape using a flathead screwdriver or a razor, separate the rear spoiler from the trunk lid.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

3. Pull the rear spoiler upward, then disengage clips A and tabs B from the trunk lid.

4. Remove the rear spoiler.

5. Install in the reverse order of removal.

  (1) Attach double-sided adhesive tape to the rear spoiler as shown in the figure.

## 5HB

1. Remove the liftgate upper trim. (SeeLIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

2. Remove the bolts and nut.

3. Pull the rear spoiler upward, then disengage clips A from the liftgate.

4. Remove the rear spoiler.

5. Install in the reverse order of removal.