CONDENSER REMOVAL/INSTALLATION

#
CONDENSER REMOVAL/INSTALLATION

B3E071161480W01

1.• Disconnect the negative battery cable.

2. Discharge the refrigerant. (See REFRIGERANT CHARGING.)

3. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT.)

4. Remove the fresh air duct cover. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [LF].)

5. Remove the fresh air duct. (Z6, ZJ) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].)

6. Remove the air cleaner. (LF) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [LF].)

7. Remove the splash shield.

8. Drain the ATF. (ATX) (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT.)

9. Disconnect the cooler hose(HI) and cooler pipe. Do not allow remaining compressor oil in the refrigerant line to spill.

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise or other malfunction could occur. Always plug open fittings immediately after removing any refrigeration cycle parts.

10. Disconnect the radiator hose from the radiator.

11. Disconnect the oil hose from the oil cooler. (ATX)

12. Remove the cooling fan. (See RADIATOR REMOVAL/INSTALLATION.)

13. Remove the oil cooler. (ATX) (See OIL COOLER REMOVAL/INSTALLATION (AUTOMATIC TRANSAXLE) [Z6].)

14. Remove the radiator with the condenser installed. (See RADIATOR REMOVAL/INSTALLATION.)

15. Release the radiator hook and pull the condenser up, being careful not to allow remaining compressor oil in the condenser to spill. (See Condenser Installation Note.)

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise or other malfunction could occur. Always plug open fittings immediately after removing any refrigeration cycle parts.

16. Install in the reverse order of removal.

17. Perform the refrigerant system performance test. (See REFRIGERANT SYSTEM PERFORMANCE TEST.)

## Condenser Installation Note

1.• After replacing the condenser, add compressor oil to the refrigeration cycle.

  Supplemental oil amount (approx. quantity)
  20 ml {20 cc, 0.7 fl oz}