REAR DOOR LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION

#
REAR DOOR LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION

B3E091458490W03

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Sail garnish (5HB) (See SAIL GARNISH REMOVAL/INSTALLATION.)
  (2) Rear door garnish (5HB) (See REAR DOOR GARNISH REMOVAL/INSTALLATION.)
  (3) Regulator handle (vehicles with manual window system) (See REGULATOR HANDLE REMOVAL.) (See REGULATOR HANDLE INSTALLATION.)
  (4) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)
  (5) Rear door glass (See REAR DOOR GLASS REMOVAL/INSTALLATION.)
  (6) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)
  (7) Inner handle (See INNER HANDLE REMOVAL/INSTALLATION.)
  (8) Rear door unit (See REAR DOOR UNIT REMOVAL/INSTALLATION.)

3. Pull the stopper of the rear door lock actuator connector in the direction of the arrow (1).

4. Disconnect the rear door lock actuator connector while pushing at point A.

5. Remove the rear door latch and lock actuator from the rear door unit.

6. Install in the reverse order of removal.