BATTERY REMOVAL/INSTALLATION [LF]

#
BATTERY REMOVAL/INSTALLATION [LF]

B3E011718520W02

1. Remove in the order indicated in the table.

  Note

  • Remove the parts 8 to 11 in the table if necessary.

2. Install in the reverse order of removal.

.

1 | Battery cover (See Battery Cover Installation Note.)
2 | Negative battery cable
3 | Positive battery cable
4 | Battery duct (See Battery Duct Installation Note.)
5 | Battery box (See Battery Box Installation Note.)
6 | Battery clamp
7 | Battery
8 | Set bolt (See Set Bolt Removal Note.) (See Set Bolt Installation Note.)
9 | PCM cover (See PCM Cover Installation Note (L.H.D.).) (See PCM Cover Installation Note (R.H.D.).)
10 | Connectors
11 | Battery tray and PCM component

## Set Bolt Removal Note

1. Drill the set bolts using a drill bit with a diameter larger than the shanks until the heads are removed.

  • If the shanks remain, remove them using locking pliers.

2. Clean all foreign material from the PCM connectors.

## PCM Cover Installation Note (L.H.D.)

1. Install with the PCM cover hooks B aligned with the PCM box holes.

2. Install the PCM cover to the PCM box hook.

## PCM Cover Installation Note (R.H.D.)

1. Insert the tab of the PCM cover to the hole.

2. Rotate until the area F is paralleled. The harness and the PCM cover should be located at the area G.

## Set Bolt Installation Note

1. Install new set bolts and temporarily tighten them first, then tighten them until the necks of the bolts break off.

## Battery Box Installation Note

1. Assemble with the battery box hooks E aligned with the battery tray holes at two points.

## Battery Duct Installation Note

1. Match the mark of the shroud panel and notch in the battery duct, and install the battery duct to the shroud panel.

## Battery Cover Installation Note

1. Install the battery duct between the battery cover and the battery box.

2. Install with the battery cover hooks A aligned with the battery tray holes at two points.

3. Install with the battery cover hooks D aligned with the battery tray flange at two points.

4. Set the battery cover to the battery tray hooks C at two points.