STARTER REMOVAL/INSTALLATION [LF]

#
STARTER REMOVAL/INSTALLATION [LF]

B3E011918400W04

  Warning

  • When the battery cables are connected, touching the vehicle body with starter terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the negative battery cable before performing the following operation.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the under cover.

4. Remove the clutch release cylinder. (MTX) (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [G35M-R].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

1 | Terminal B cable
2 | Terminal S connector
3 | Wiring harness bracket
4 | Starter