DTC P0610 [ZJ, Z6]

#
DTC P0610 [ZJ, Z6]

B3E010200600W02

DTC P0610 | PCM vehicle options error
--- | ---

DETECTION CONDITION

• PCM data configuration error.
Diagnostic support note
• This is a continuous monitor (CCM).
• The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle.
• PENDING CODE is available if the PCM detects the above malfunction condition.
• FREEZE FRAME DATA is available.
• The DTC is stored in the PCM memory.

POSSIBLE CAUSE | • Configuration procedure has not been completed • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Perform the "PCM CONFIGURATION", then go to the next step. (See PCM CONFIGURATION [ZJ, Z6].)
3 | VERIFY TROUBLESHOOTING OF DTC P0610 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [ZJ, Z6].)
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [ZJ, Z6].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [ZJ, Z6].)
No | DTC troubleshooting completed.