CLUTCH PEDAL POSITION (CPP) SWITCH INSPECTION [ZJ, Z6]

#
CLUTCH PEDAL POSITION (CPP) SWITCH INSPECTION [ZJ, Z6]

B3E014018660W02

  Note

  • Before performing the following inspection, make sure to follow the procedure as indicated in the troubleshooting flowchart. (See Troubleshooting Procedure.)

## Continuity Inspection

1. Remove the CPP switch.

2. Verify that the continuity between CPP switch terminals A and B is as indicated in the table.

  • If not as indicated in the table, replace the CPP switch. (See CLUTCH PEDAL REMOVAL/INSTALLATION.)
  • If the monitor item condition/specification (reference) is not within the specification, even though there is no malfunction, perform the "Circuit Open/Short Inspection".

## Circuit Open/Short Inspection

1. Remove the PCM connector cover.

2. Disconnect the PCM connector. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].)

3. Inspect the following wiring harness for open or short circuit (continuity check).

### Open circuit

  • If there is no continuity, there is an open circuit. Repair or replace the wiring harness.
  - CPP switch terminal A and PCM terminal 1P
  - CPP switch terminal B and body GND

### Short circuit

  • If there is continuity, there is a short circuit. Repair or replace the wiring harness.
  - CPP switch terminal A and body GND
  - CPP switch terminal B and power supply