ON-BOARD DIAGNOSTIC TEST [ZJ, Z6]

#
ON-BOARD DIAGNOSTIC TEST [ZJ, Z6]

B3E010200102W19

## DTC Reading Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Retrieve the DTCs using the WDS or equivalent.

## Pending Trouble Code Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Retrieve the pending trouble codes using the WDS or equivalent.

## Freeze Frame PID Data Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Record the freeze frame PID data using the WDS or equivalent.

## On-Board System Readiness Tests Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Monitor the OBD systems operating status using the WDS or equivalent.

## PID/DATA Monitor and Record Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Access and monitor PIDs using the WDS or equivalent.

## Diagnostic Monitoring Test Results Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Access to the diagnostic monitoring test results and read the test results using the WDS or equivalent.