NO.22 VIBRATION CONCERNS (ENGINE) [LF]

#
NO.22 VIBRATION CONCERNS (ENGINE) [LF]

B3E010318881W24

22 | VIBRATION CONCERNS (ENGINE)
--- | ---
DESCRIPTION | • Vibration from under hood or driveline
POSSIBLE CAUSE | • Loose attaching bolts or worn parts • Components malfunction such as worn parts

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---

1

Inspect the following components for loose attaching bolts or worn parts:
• Cooling fan
• Drive belt and pulleys
• Generator
• Engine mounts
• Exhaust system mounts
All items normal?

Yes

Inspect following systems:
• Wheels
• Driveline
• Suspension

No | Readjust or retighten engine mount installation position. Service if necessary for other parts.

2

Verify test results.
• If normal, return to diagnostic index to service any additional symptoms.
(See ENGINE SYMPTOM TROUBLESHOOTING [LF].)
• If malfunction remains, inspect related Service information perform repair or diagnosis.

  - If vehicle repaired, troubleshooting completed.
  - If vehicle not repaired or additional diagnostic information not available, replace the PCM.
  (See PCM REMOVAL/INSTALLATION [LF].)