TRANSMISSION/TRANSAXLE TECHNICAL DATA

#
TRANSMISSION/TRANSAXLE TECHNICAL DATA

B3E055001024W01

Item | Specifications
--- | ---
CLUTCH
Clutch pedal | Disengagement point | Disengagement stroke | (mm {in}) | 90-110 {3.55-4.33} (Reference value)
Pedal stroke | (mm {in}) | 135 {5.31} (Reference value)
Clutch cover | Diaphragm spring fingers | Depth | (mm {in}) | 0.6 {0.024}
Maximum height difference | (mm {in}) | 1.0 {0.039}
Maximum clearance of flatness of the pressure plate | (mm {in}) | 0.5 {0.020}
Clutch disc | Minimum depth | (mm {in}) | 0.3 {0.012}
Maximum runout | (mm {in}) | 0.7 {0.028}
Flywheel | Maximum runout | (mm {in}) | 0.1 {0.004}
Clutch fluid | Type |  | SAE J1703, FMVSS 116 DOT-3 or DOT-4
MANUAL TRANSAXLE
Engine type | ZJ, Z6
Manual transaxle type | F35M-R
Oil | Grade | API Service GL-4 or GL-5
Viscosity | All-season | SAE 75W-90
Above 10 °C {50 °F} | SAE 80W-90
Capacity (Approximate quantity) | 3.04 {3.21, 2.67}
(L {US qt, lmp qt})
Engine type | LF
Manual transaxle type | G35M-R
Oil | Grade | API Service GL-4 or GL-5
Viscosity | All-season | SAE 75W-90
Above 10 °C {50 °F} | SAE 80W-90
Capacity (Approximate quantity) | 2.87 {3.03, 2.53}
(L {US qt, lmp qt})
AUTOMATIC TRANSAXLE
Engine type | Z6 | LF
Automatic transaxle type | FN4A-EL
ATF | Type | ATF M-V
Capacity (Approx. quantity) | 7.0 {7.4, 6.2} | 7.2 {7.6, 6.3}
(L {US qt, lmp qt})
Line pressure | D, M (1GR, 2GR) range | Idle | 330-470 {3.4-4.7, 48-68}
Stall | 1,090-1,250 {11.2-12.7, 159-181} | 1,160-1,320 {11.8-13.5, 168-191}
(kPa {kgf/cm2, psi}) | R position | Idle | 490-710 {5.0-7.2, 72-102}
Stall | 1,470-1,690 {15.0-17.2, 214-245} | 1,600-1,820 {16.4-18.5, 234-263}
Engine stall speed | (rpm) | D, M range | 2,100-2,700 | 2,000-2,600
R position
Time lag | (s) | N position→ D range | 0.4-0.7
N position→ R position | 0.4-0.7
Transaxle range (TR) switch | (ohm) | P position | 4,085-4,515
R position | 1,425-1,575
N position | 713-788
D range | 371-409
Transaxle Fluid temperature (TFT) sensor | (kilohm) | ATF temperature: -20 °C {-4 °F} | 236-324
ATF temperature: 0 °C {32 °F} | 84.3-110
ATF temperature: 20 °C {68 °F} | 33.5-42.0
ATF temperature: 40 °C {104 °F} | 14.7-17.9
ATF temperature: 60 °C {140 °F} | 7.08-8.17
ATF temperature: 80 °C {176 °F} | 3.61-4.15
ATF temperature: 100 °C {212 °F} | 1.96-2.24
ATF temperature: 120 °C {248 °F} | 1.13-1.28
ATF temperature: 130 °C {266 °F} | 0.87-0.98
Input/turbine speed sensor | (ohm) | ATF temperature: -40-160 °C {-40-320 °F} | 250-600
Vehicle speed sensor (VSS) | (V) | 4.5-5.5
Solenoid valves ATF temperature: -40-150 °C {-40-302 °F} | (ohm) | Shift solenoid A | 1.0-4.2
Shift solenoid B | 1.0-4.2
Shift solenoid C | 1.0-4.2
Shift solenoid D | 10.9-26.2
Shift solenoid F | 10.9-26.2
Pressure control | 2.4-7.3