IGNITION COIL INSPECTION [ZJ, Z6]

#
IGNITION COIL INSPECTION [ZJ, Z6]

B3E011801009W05

## Ignition Coil Inspection

  Note

  • It is unlikely that all four ignition coils fail to operate properly. To prevent replacing a normal component, perform the following procedure, identify the malfunctioning ignition coil, and replace it.

1. Perform the spark test and identify the malfunctioning cylinder.

2. Replace the ignition coil of the malfunctioning cylinder with that of a normal cylinder, and reperform the spark test.

  • If the spark is not normal due to a malfunctioning ignition coil, replace that ignition coil.

## Ignition Coil with Built-In Power Switch Inspection

1. Remove the ignition coil connector.

2. Measure the resistance between each terminal on the ignition coil connector.

  • If the measurement corresponds to the table, replace the ignition coil.

Item | Tester Connection Position | Condition
--- | --- | ---
Positive | Negative
Terminal | C | B | ∞ or 0 ohm is not normal
A | B
A | C | 0 to several kilohms (continuity) is not normal