STEERING

#
STEERING

B3E065001034W01

Item | Specification
--- | ---
POWER STEERING
Steering wheel | Play | (mm {in}) | 0-30 {0-1.18}
Effort | (N·m {kgf·cm, in·lbf}) | 7.8 {80, 69} max. (reference value)
Steering shaft | Standard length | (mm {in}) | 315-320 {12.41-12.59}
Steering gear | Tie-rod end | Rotation torque | (N·m {kgf·cm, in·lbf}) | 0.5-3.0 {6-30, 5-26}
Tie rod | Swinging torque | (N·m {kgf·cm, in·lbf}) | 0.4-4.0 {5-40, 4-35}
[Pull scale reading] | (N {kgf, lbf}) | 0.6-29.3 {0.06-2.98, 0.14-6.58}
Steering rack | Runout | Large diameter portion | 0.15 {0.006} max.
(mm {in}) | Small diameter portion | 0.20 {0.008} max.
Power steering oil pump | Oil pump fluid pressure | (MPa {kgf·cm2, psi}) | 8.5-9.0 {87-91, 1235-1305} (ZJ, Z6) 10.4-11.0 {107-112, 1509-1595} (LF)
Gear housing fluid pressure | (MPa {kgf·cm2, psi}) | 7.6-9.0 {78-91, 1103-1305} (ZJ, Z6) 9.0-11.0 {92-111, 1306-1585} (LF)
Power steering system | Fluid | Type | ATF M-III or equivalent (e.g. DexronII)
Capacity* (Approximate quantity) | (L {US qt, Imp qt}) | 1.20 {1.27, 1.06} (ZJ, Z6) 0.80 {0.84, 0.70} (LF)

  * :
When reserve tank is at maximum volume