AIR INTAKE ACTUATOR INSPECTION

#
AIR INTAKE ACTUATOR INSPECTION

B3E074061060W02

1. Connect battery positive voltage to air intake actuator terminal C (or G), connect terminal G (or E) to ground, and then verify that the air intake actuator operates as shown in the table.

  • If the operation condition is not normal, replace the air intake actuator.

L.H.D.

Terminal | Air intake actuator operation
--- | ---
C | E | G
B+ | - | Ground | FRESH→RECIRCULATE
- | Ground | B+ | RECIRCULATE→FRESH