DTC 00:ER04

#
DTC 00:ER04

B3E090266900W16

DTC 00:Er04 | Cassette tape

DETECTION CONDITION

  Note

  • When error occurs, error message "CHECK TAPE" is displayed in the LCD.

• Cassette tape is worn out.

POSSIBLE CAUSE | • Tape wear • Cassette deck malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Verify condition of the cassette tape when the error occurs. Is the cassette tape normal? | Yes | Go to the next step.
No | Replace the cassette tape and go to the next step.
2 | Clear the DTC, and then insert a normal cassette tape. Play the cassette tape for 20 s or more. Is DTC 00: Er04 displayed? | Yes | Replace the cassette deck.
No | DTC troubleshooting completed.