TRUNK SIDE TRIM REMOVAL/INSTALLATION

#
TRUNK SIDE TRIM REMOVAL/INSTALLATION

B3E0917688T0W01

## 4SD

1. Remove the following parts:

  (1) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)
  (5) Service hole cover (LH)

2. Remove the fasteners, then remove the trunk side trim.

3. Install in the reverse order of removal.

## 5HB

1. Remove the following parts:

  (1) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)
  (5) Trunk side upper trim (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION.)
  (6) Cargo compartment light (See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION.)

2. Remove the screws, then remove the trunk board.

3. Remove the screws, then remove the cargo net hooks.

4. Remove the fasteners.

5. Detach the clip A and remove the trunk side trim.

6. Install in the reverse order of removal.