BRAKE SWITCH INSPECTION

#
BRAKE SWITCH INSPECTION

B3E041166490W02

  Caution

  • Inspect the brake switch with it installed to the brake pedal, otherwise the brake switch may not operate normally. If the brake switch is removed from the brake pedal, replace the brake switch with a new one.

1. Remove the lower panel.

2. Remove the column cover.

3. Disconnect the brake switch connector.

4. Verify that the continuity is as indicated in the table.

  • If not as indicated in the table, replace the brake switch.